| CMSIS-CORE Version 3.01 CMSIS-CORE support for Cortex-M processor-based devices

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

Data Fields
DWT_Type Struct Reference

Structure type to access the Data Watchpoint and Trace Register (DWT).

## Data Fields
__IO uint32_t | CTRL
| Offset: 0x000 (R/W) Control Register.
__IO uint32_t | CYCCNT
| Offset: 0x004 (R/W) Cycle Count Register.
__IO uint32_t | CPICNT
| Offset: 0x008 (R/W) CPI Count Register.
__IO uint32_t | EXCCNT
| Offset: 0x00C (R/W) Exception Overhead Count Register.
__IO uint32_t | SLEEPCNT
| Offset: 0x010 (R/W) Sleep Count Register.
__IO uint32_t | LSUCNT
| Offset: 0x014 (R/W) LSU Count Register.
__IO uint32_t | FOLDCNT
| Offset: 0x018 (R/W) Folded-instruction Count Register.
__I uint32_t | PCSR
| Offset: 0x01C (R/ ) Program Counter Sample Register.
__IO uint32_t | COMP0
| Offset: 0x020 (R/W) Comparator Register 0.
__IO uint32_t | MASK0
| Offset: 0x024 (R/W) Mask Register 0.
__IO uint32_t | FUNCTION0
| Offset: 0x028 (R/W) Function Register 0.
uint32_t | RESERVED0 [1]
| Reserved.
__IO uint32_t | COMP1
| Offset: 0x030 (R/W) Comparator Register 1.
__IO uint32_t | MASK1
| Offset: 0x034 (R/W) Mask Register 1.
__IO uint32_t | FUNCTION1
| Offset: 0x038 (R/W) Function Register 1.
uint32_t | RESERVED1 [1]
| Reserved.
__IO uint32_t | COMP2
| Offset: 0x040 (R/W) Comparator Register 2.
__IO uint32_t | MASK2
| Offset: 0x044 (R/W) Mask Register 2.
__IO uint32_t | FUNCTION2
| Offset: 0x048 (R/W) Function Register 2.
uint32_t | RESERVED2 [1]
| Reserved.
__IO uint32_t | COMP3
| Offset: 0x050 (R/W) Comparator Register 3.
__IO uint32_t | MASK3
| Offset: 0x054 (R/W) Mask Register 3.
__IO uint32_t | FUNCTION3
| Offset: 0x058 (R/W) Function Register 3.

## Field Documentation

__IO uint32_t DWT_Type::COMP0

__IO uint32_t DWT_Type::COMP1

__IO uint32_t DWT_Type::COMP2

__IO uint32_t DWT_Type::COMP3

__IO uint32_t DWT_Type::CPICNT

__IO uint32_t DWT_Type::CTRL

__IO uint32_t DWT_Type::CYCCNT

__IO uint32_t DWT_Type::EXCCNT

__IO uint32_t DWT_Type::FOLDCNT

__IO uint32_t DWT_Type::FUNCTION0

__IO uint32_t DWT_Type::FUNCTION1

__IO uint32_t DWT_Type::FUNCTION2

__IO uint32_t DWT_Type::FUNCTION3

__IO uint32_t DWT_Type::LSUCNT

__IO uint32_t DWT_Type::MASK0

__IO uint32_t DWT_Type::MASK1

__IO uint32_t DWT_Type::MASK2

__IO uint32_t DWT_Type::MASK3

__I uint32_t DWT_Type::PCSR

uint32_t DWT_Type::RESERVED0[1]

uint32_t DWT_Type::RESERVED1[1]

uint32_t DWT_Type::RESERVED2[1]

__IO uint32_t DWT_Type::SLEEPCNT