| CMSIS-DSP Verison 1.1.0 CMSIS DSP Software Library

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Reference

arm_signal_converge_example_f32.c

    /* ----------------------------------------------------------------------
    * Copyright (C) 2010 ARM Limited. All rights reserved.
    *
    * $Date:        29. November 2010
    * $Revision:    V1.0.3
    *
    * Project:          CMSIS DSP Library
    * Title:            arm_signal_converge_example_f32.c
    *
    * Description:  Example code demonstrating convergence of an adaptive
    *               filter.
    *
    * Target Processor: Cortex-M4/Cortex-M3
    *
    *
    * Version 1.0.3 2010/11/29
    *    Re-organized the CMSIS folders and updated documentation.
    *
    * Version 1.0.1 2010/10/05 KK
    *    Production release and review comments incorporated.
    *
    * Version 1.0.0 2010/09/20 KK
    *    Production release and review comments incorporated.
    * ------------------------------------------------------------------- */

    #include "arm_math.h"
    #include "math_helper.h"

    /* ----------------------------------------------------------------------
    ** Global defines for the simulation
    * ------------------------------------------------------------------- */

    #define TEST_LENGTH_SAMPLES 1536
    #define NUMTAPS                         32
    #define BLOCKSIZE                       32
    #define DELTA_ERROR         0.000001f
    #define DELTA_COEFF         0.0001f
    #define MU                                      0.5f

    #define NUMFRAMES (TEST_LENGTH_SAMPLES / BLOCKSIZE)

    /* ----------------------------------------------------------------------
    * Declare FIR state buffers and structure
    * ------------------------------------------------------------------- */

    float32_t firStateF32[NUMTAPS + BLOCKSIZE];
    arm_fir_instance_f32 LPF_instance;

    /* ----------------------------------------------------------------------
    * Declare LMSNorm state buffers and structure
    * ------------------------------------------------------------------- */

    float32_t lmsStateF32[NUMTAPS + BLOCKSIZE];
    float32_t errOutput[TEST_LENGTH_SAMPLES];
    arm_lms_norm_instance_f32 lmsNorm_instance;

    /* ----------------------------------------------------------------------
    * Function Declarations for Signal Convergence Example
    * ------------------------------------------------------------------- */

    arm_status test_signal_converge_example( void );

    /* ----------------------------------------------------------------------
    * Internal functions
    * ------------------------------------------------------------------- */
    arm_status test_signal_converge(float32_t* err_signal,
                                                         uint32_t blockSize);

    void getinput(float32_t* input,
                     uint32_t fr_cnt,
                 uint32_t blockSize);

    /* ----------------------------------------------------------------------
    * External Declarations for FIR F32 module Test
    * ------------------------------------------------------------------- */
    extern float32_t testInput_f32[TEST_LENGTH_SAMPLES];
    extern float32_t lmsNormCoeff_f32[32];
    extern const float32_t FIRCoeff_f32[32];
    extern arm_lms_norm_instance_f32 lmsNorm_instance;

    /* ----------------------------------------------------------------------
    * Declare I/O buffers
    * ------------------------------------------------------------------- */

    float32_t wire1[BLOCKSIZE];
    float32_t wire2[BLOCKSIZE];
    float32_t wire3[BLOCKSIZE];
    float32_t err_signal[BLOCKSIZE];

    /* ----------------------------------------------------------------------
    * Signal converge test
    * ------------------------------------------------------------------- */

    int32_t main(void)
    {
      uint32_t i;
      arm_status status;
      uint32_t index;
      float32_t minValue;

      /* Initialize the LMSNorm data structure */
      arm_lms_norm_init_f32(&lmsNorm_instance, NUMTAPS, lmsNormCoeff_f32, lmsStateF32, MU, BLOCKSIZE);

      /* Initialize the FIR data structure */
      arm_fir_init_f32(&LPF_instance, NUMTAPS, (float32_t *)FIRCoeff_f32, firStateF32, BLOCKSIZE);

      /* ----------------------------------------------------------------------
      * Loop over the frames of data and execute each of the processing
      * functions in the system.
      * ------------------------------------------------------------------- */

      for(i=0; i < NUMFRAMES; i++)
        {
          /* Read the input data - uniformly distributed random noise - into wire1 */
          arm_copy_f32(testInput_f32 + (i * BLOCKSIZE), wire1, BLOCKSIZE);

          /* Execute the FIR processing function.  Input wire1 and output wire2 */
          arm_fir_f32(&LPF_instance, wire1, wire2, BLOCKSIZE);

          /* Execute the LMS Norm processing function*/

          arm_lms_norm_f32(&lmsNorm_instance, /* LMSNorm instance */
                           wire1,                     /* Input signal */
                           wire2,                             /* Reference Signal */
                           wire3,                             /* Converged Signal */
                           err_signal,                        /* Error Signal, this will become small as the signal converges */
                           BLOCKSIZE);                        /* BlockSize */

          /* apply overall gain */
          arm_scale_f32(wire3, 5, wire3, BLOCKSIZE);         /* in-place buffer */
        }

      status = ARM_MATH_SUCCESS;

      /* -------------------------------------------------------------------------------
      * Test whether the error signal has reached towards 0.
      * ----------------------------------------------------------------------------- */

      arm_abs_f32(err_signal, err_signal, BLOCKSIZE);
      arm_min_f32(err_signal, BLOCKSIZE, &minValue, &index);

      if (minValue > DELTA_ERROR)
      {
          status = ARM_MATH_TEST_FAILURE;
      }

      /* ----------------------------------------------------------------------
      * Test whether the filter coefficients have converged.
      * ------------------------------------------------------------------- */

      arm_sub_f32((float32_t *)FIRCoeff_f32, lmsNormCoeff_f32, lmsNormCoeff_f32, NUMTAPS);

      arm_abs_f32(lmsNormCoeff_f32, lmsNormCoeff_f32, NUMTAPS);
      arm_min_f32(lmsNormCoeff_f32, NUMTAPS, &minValue, &index);

      if (minValue > DELTA_COEFF)
      {
          status = ARM_MATH_TEST_FAILURE;
      }

      /* ----------------------------------------------------------------------
      * Loop here if the signals did not pass the convergence check.
      * This denotes a test failure
      * ------------------------------------------------------------------- */

      if( status != ARM_MATH_SUCCESS)
      {
          while(1);
      }

        while(1);                             /* main function does not return */
    }