; generated by Component: ARM Compiler 5.05 update 2 (build 169) Tool: ArmCC [4d0f38]
; commandline ArmCC [--list --debug -c --asm --interleave -o.\obj\main.o --asm_dir=.\lst\ --list_dir=.\lst\ --depend=.\obj\main.d --cpu=Cortex-M4.fp --apcs=interwork -O0 --diag_suppress=9931 -I..\..\..\Library\CMSIS\Include -I..\..\..\Library\Device\Nuvoton\M451Series\Include -I..\..\..\Library\StdDriver\inc -I..\Bsp -I..\User -I..\touch_driver -I.\RTE\_project -IC:\Keil_v5\ARM\PACK\ARM\CMSIS\4.3.0\CMSIS\Include -IDevice\M451\Include -D__UVISION_VERSION=527 -D_RTE_ --omf_browse=.\obj\main.crf ..\User\main.c]
                          THUMB

                          AREA ||.text||, CODE, READONLY, ALIGN=2

                  main PROC
;;;34     *******************************************************************************/
;;;35     int main(void)
000000  bf00              NOP      
000002  bf00              NOP      
000004  bf00              NOP      
                  |L1.6|
000006  2059              MOVS     r0,#0x59
000008  490c              LDR      r1,|L1.60|
00000a  6008              STR      r0,[r1,#0]
00000c  2016              MOVS     r0,#0x16
00000e  0589              LSLS     r1,r1,#22
000010  f8c10100          STR      r0,[r1,#0x100]
000014  2088              MOVS     r0,#0x88
000016  f8c10100          STR      r0,[r1,#0x100]
00001a  06c0              LSLS     r0,r0,#27
00001c  f8d00100          LDR      r0,[r0,#0x100]
000020  2800              CMP      r0,#0
000022  d0f0              BEQ      |L1.6|
000024  bf00              NOP      
;;;36     {
;;;37     	/* Unlock protected registers */
;;;38     	SYS_UnlockReg();
;;;39     	SYS_Init();
000026  f7fffffe          BL       SYS_Init
;;;40     	/* Lock protected registers */
;;;41     	SYS_LockReg();
00002a  bf00              NOP      
00002c  2000              MOVS     r0,#0
00002e  4903              LDR      r1,|L1.60|
000030  6008              STR      r0,[r1,#0]
000032  bf00              NOP      
;;;42     		
;;;43     	VK3816_Main();
000034  f7fffffe          BL       VK3816_Main
;;;44     	
;;;45     	while(1)
000038  bf00              NOP      
                  |L1.58|
00003a  e7fe              B        |L1.58|
;;;46     	{					
;;;47     	}
;;;48     }	
;;;49     /************************END OF FILE****/
                          ENDP

                  |L1.60|
                          DCD      0x40000100

;*** Start embedded assembler ***

#line 1 "..\\User\\main.c"
	AREA ||.rev16_text||, CODE
	THUMB
	EXPORT |__asm___6_main_c_main____REV16|
#line 114 "..\\..\\..\\Library\\CMSIS\\Include\\core_cmInstr.h"
|__asm___6_main_c_main____REV16| PROC
#line 115

 rev16 r0, r0
 bx lr
	ENDP
	AREA ||.revsh_text||, CODE
	THUMB
	EXPORT |__asm___6_main_c_main____REVSH|
#line 128
|__asm___6_main_c_main____REVSH| PROC
#line 129

 revsh r0, r0
 bx lr
	ENDP

;*** End   embedded assembler ***

                  __ARM_use_no_argv EQU 0
