| CMSIS-RTOS Version 1.00 CMSIS-RTOS API: Generic RTOS interface for Cortex-M processor-based devices.

- CMSIS
- CORE
- DSP
- RTOS API
- SVD

- Main Page
- Usage and Description
- Reference

Defines | Functions
Memory Pool Management
CMSIS-RTOS API

Define and manage fixed-size memory pools. More...

## Defines
#define | osFeature_Pool 1
| Memory Pools: 1=available, 0=not available.
#define | osPoolDef(name, no, type)
| Define a Memory Pool.
#define | osPool(name) &os_pool_def_##name
| Access a Memory Pool definition.
## Functions
osPoolId | osPoolCreate (osPoolDef_t *pool_def)
| Create and Initialize a memory pool.
void * | osPoolAlloc (osPoolId pool_id)
| Allocate a memory block from a memory pool.
void * | osPoolCAlloc (osPoolId pool_id)
| Allocate a memory block from a memory pool and set memory block to zero.
osStatus | osPoolFree (osPoolId pool_id, void *block)
| Return an allocated memory block back to a specific memory pool.

## Description

The Memory Pool Management function group is used to define and manage fixed-sized memory pools.

## Define Documentation

#define osFeature_Pool 1

A CMSIS-RTOS implementation may support fixed-size memory pools. When the value osFeature_Pool is 1 memory pools are supported. When the value osFeature_Pool is 0 no memory pools are supported.

#define osPool | ( |  | name | ) | &os_pool_def_##name

Access a memory pool for the functions osPoolCreate.

Parameters:

  name | name of the memory pool

Note:
  CAN BE CHANGED: The parameter to osPool shall be consistent but the macro body is implementation specific in every CMSIS-RTOS.

#define osPoolDef | ( |  | name,
|  |  | no,
|  |  | type
| ) |  |

Define a memory pool that is referenced by osPool.

Parameters:

  name | name of the memory pool.
  no | maximum number of objects (elements) in the memory pool.
  type | data type of a single object (element).

Note:
  CAN BE CHANGED: The parameter to osPoolDef shall be consistent but the macro body is implementation specific in every CMSIS-RTOS.

## Function Documentation

void * osPoolAlloc | ( | osPoolId | pool_id | ) |

Parameters:

  [in] | pool_id | memory pool ID obtain referenced with osPoolCreate.

Returns:
  address of the allocated memory block or NULL in case of no memory available.

Note:
  MUST REMAIN UNCHANGED: osPoolAlloc shall be consistent in every CMSIS-RTOS.

Allocate a memory block from the memory pool.

void * osPoolCAlloc | ( | osPoolId | pool_id | ) |

Parameters:

  [in] | pool_id | memory pool ID obtain referenced with osPoolCreate.

Returns:
  address of the allocated memory block or NULL in case of no memory available.

Note:
  MUST REMAIN UNCHANGED: osPoolCAlloc shall be consistent in every CMSIS-RTOS.

Allocate a memory block from the memory pool. The block is initialized to zero.

osPoolId osPoolCreate | ( | osPoolDef_t * | pool_def | ) |

Parameters:

  [in] | pool_def | memory pool definition referenced with osPool.

Returns:
  memory pool ID for reference by other functions or NULL in case of error.

Note:
  MUST REMAIN UNCHANGED: osPoolCreate shall be consistent in every CMSIS-RTOS.

Create and initialize a memory pool.

osStatus osPoolFree | ( | osPoolId | pool_id,
|  | void * | block
| ) |  |

Parameters:

  [in] | pool_id | memory pool ID obtain referenced with osPoolCreate.
  [in] | block | address of the allocated memory block that is returned to the memory pool.

Returns:
  status code that indicates the execution status of the function.

Note:
  MUST REMAIN UNCHANGED: osPoolFree shall be consistent in every CMSIS-RTOS.

Return a memory block to a memory pool.

Status and Error Codes

- osOK: the memory block is released.
- osErrorValue: block does not belong to the memory pool.
- osErrorParameter: a parameter is invalid or outside of a permitted range.